# Techno Machine Tools

Survey no:126/A/1, DOOR NO: 4-132-9/A/2, Gandimaisamma X Road,

Medchal Malkajgeri,Hyderabad-500043.Telangana, India.

(Mfg of bailing presses)

*T.SIVARAMAKRISHNA*

# ME.,MBA.

Ref:-TM/HYD/S0299/2025 31-05-2025

To

|  |  |  |
| --- | --- | --- |
| |  | | --- | |  | | Bharath | |
| Hyderabad, Telangana, India |
| Email: [bharathk7036@gmail.com](mailto:bharathk7036@gmail.com) |
| Mobile: [+(91)-8074850768](http://indmrt.in/bevtvvlt/call+91-8074850768) |

# DearSir

SUB:-SUPPLYOFPAPERCARDBOARDBAILINGPRESS CONTINUESOPERATION

With reference to our discussions regarding your requirement of Card Board Bailing Press. We are glad to inform you that, we are in a position to supply you the required equipment. The following are the specifications and our terms and conditions.

# Specificationsoftheequipment

***TechnicalSpecifications:-***

MaxWorkingPressure - 250Kg/cm2 NormalWorkingPressure -200 Kg/cm2

DesignPressure - 250 Kg/Cm2 Tonnageat200 Kg/cm2 - 55Tons-2nos CylBore - 180 mm

RodDia - 120mm Stroke - 1600 mm

Mtg - FrontFlange

Approach Speed - 60mm/sec ReturnSpeed - 120 mm/sec

HP - 75.0HP

TankCap - 2600Ltr

*DetailBillofMaterial*

CylinderSeals -ImportedGermanSeals (MerkelorHalite)

Motor -ABB/Siemens /Kirloskar/Crompton

RodSeal -ImportedhaliteSeal

Valves -Yuken/Polyhydron/Hydrotech

CheckValves -Polyhydron

HydraulicPump -Yuken/Dowty

HighPrPump -Polyhydron

BellHousing -Micro

ReliefValves -Polyhydron HydTank - Micro

HydTank - MHPL

Fitting -Hyloc /Hydair

Gasket -Champion

Fastners - TVS/LPS

Balesize: - (w)1120X(H)1050X(L)V

Bailing chamber size - (w)1120X(H)1050X(L)2400 Feeding hopper size- (w)1120 X (L) 1825

Body - msfabricated

Bale weight - 1200–1600depends

Workingpressure- 200 bar

|  |  |
| --- | --- |
| Drive | - |
| Tyingcylinders | - |
| Noof ties | - |
| Wiresize | - |
| Baldes | - |
| Hopper | - |
| Oiltankcapacity | - |
| Operation | - |
| Chiller | - |
| Conveyer |  |
| Drive | - |
| Belt | - |
| Beltwidth | - |
| Speed | - |

75HPAND&7.5HP

provided 4 nos

3.24-4mm

provided provided

2600lts(inbuyersscope) plc

buyersscope

7.5 hpslat chain 1800 mm variable

|  |  |  |
| --- | --- | --- |
| **SNo** | **Description of the unit** | **Offer/unit** |
| 1. | Continues cardboard bailing machine with complete automatic along with above specifications | **Rs55,00,000/-**  (Fifty five Lakhs Only) |

GENERAL TERMS & CONDITIONS:

1. Price quoted per unit ex-work. Hyderabad.
2. Following charges are additional to your account.

* Freight Charge : As actual to be borne by you.
* Sales Tax : 18% Extra as applicable
* Packing charge : As actual to be borne by you.
* Insurance : As actual to be borne by you.

1. Payment : 50% advance along with order balance before delivery but after inspection at our works.
2. Delivery : Within 1 months from date of advance received
3. Validity : One month from the date of submission.
4. Inspection : Inspection at our works prior to dispatch.
5. Warranty : The machine is warranted for a period of 12 months from the date of dispatch against any manufacturing defects/ faulty material or bad workmanship of any part or component but not against any kind of abnormal or improper use of machine. Defective part or component will be replaced or repaired free of cost. Electrical components are outside the scope of this warranty.
6. Commissioning : Erection & commissioning done by you, but required technical support & guidance provide by us at additional cost.

NOTE:

1. Oil is not in scope of our supply.
2. Raw material for trial is to be arranged by you at your cost.

We are sure you will find our offer in line with your requirements. Should you require any further clarification please contact T.SIVARAMAKRISHNA 9246221106/9849207176 emil: techno9246221106@gmail.com

Thanking you and assuring you of our best services.

**For TECHNOMACHINETOOLS ( T. SIVARAMAKRISHNA)**

